Impromptu Net Notice|F!106

. Version: 06/25/2025 - @SITREP

# Release date 20250323 - KN4AM - @SITREP - SitRepNet.com
# Updated 20250422, 20250625

! Impromptu Net Notice - @SITREP

. Impromptu, special purpose net to address a specific event.
.
[DS] Brief description of net purpose:
? Expected duration of this net series:
@1 One time net
@2 Unknown / indefinite
.

!!! Scheduled Date/Time:
? Date - current or following month:
@A 01
@B 02
@C 03
@D 04
@E 05
@F 06
@G 07
@H 08
@I 09
@J 10
@K 11
@L 12
@M 13
@N 14
@O 15
@P 16
@Q 17
@R 18
@S 19
@T 20
@U 21
@V 22
@W 23
@X 24
@Y 25
@Z 26
@1 27
@2 28
@3 29
@4 30
@5 31
@6 See Additional Info.

? Time standard:
@L Local time
@Z Zulu (UTC/GMT)

? Scheduled HOUR start time of net:
@A 01:00
@B 02:00
@C 03:00
@D 04:00
@E 05:00
@F 06:00
@G 07:00
@H 08:00
@I 09:00
@J 10:00
@K 11:00
@L 12:00
@M 13:00
@N 14:00
@O 15:00
@P 16:00
@Q 17:00
@R 18:00
@S 19:00
@T 20:00
@U 21:00
@V 22:00
@W 23:00
@X 24:00

? Scheduled MINUTE start time of net:
@A 00
@B 05
@C 10
@F 15
@E 20
@F 25
@G 30
@H 35
@I 40
@J 45
@K 50
@L 55

? Early Check-ins?
@N No - Net starts at specified time
@Y Yes - Early check-ins accepted
@U Unknown at this time
.

!!! Net Operations

? Mode at start of net:
@J JS8
@C Contestia 4/250
@M MFSK-32
@V Voice
@O Other - See Additional Information field

? Frequency for this impromptu net:
@0 None of these - See Additional Information field
@A Built-in JS8Call Standard 80m, 3.578 MHz
@B 80m 3.585 MHz
@C 80m 3.588 MHz
@D Built-in JS8Call Standard 40m, 7.078 MHz
@E 40m 7.107 MHz
@F 40m 7.110 MHz
@G 40m 7.115 MHz
@H Built-in JS8Call Standard 20m, 14.078 MHz
@I 20m 14.107 MHz
@J 20m 14.110 MHz
@K 20m 14.115 MHz
. Set Waterfall to 900 for FLDIGI, 2300 for JS8Call unless otherwise specified.
.

[AI] Additional Information:


. ________________________________________________________________________
. For impromptu / event-driven nets.
